From: Daniel Golle <daniel@makrotopia.org>
Subject: [PATCH] ath79: add support for Atheros AR934x HS UART

AR934x chips also got the 'old' qca,ar9330-uart in addition to the
'new' ns16550a compatible one. Add support for UART1 clock selector as
well as device-tree bindings in ar934x.dtsi to make use of that uart.

Reported-by: Piotr Dymacz <pepe2k@gmail.com>
Submitted-by: Daniel Golle <daniel@makrotopia.org>
---
 arch/mips/ath79/clock.c                       | 7 +++++++
 .../mips/include/asm/mach-ath79/ar71xx_regs.h | 1 +
 include/dt-bindings/clock/ath79-clk.h         | 3 ++-
 3 files changed, 10 insertions(+), 1 deletion(-)

--- a/arch/mips/ath79/clock.c
+++ b/arch/mips/ath79/clock.c
@@ -40,6 +40,7 @@ static const char * const clk_names[ATH7
 	[ATH79_CLK_AHB] = "ahb",
 	[ATH79_CLK_REF] = "ref",
 	[ATH79_CLK_MDIO] = "mdio",
+	[ATH79_CLK_UART1] = "uart1",
 };
 
 static const char * __init ath79_clk_name(int type)
@@ -344,6 +345,9 @@ static void __init ar934x_clocks_init(vo
 	if (clk_ctrl & AR934X_PLL_SWITCH_CLOCK_CONTROL_MDIO_CLK_SEL)
 		ath79_set_clk(ATH79_CLK_MDIO, 100 * 1000 * 1000);
 
+	if (clk_ctrl & AR934X_PLL_SWITCH_CLOCK_CONTROL_UART1_CLK_SEL)
+		ath79_set_clk(ATH79_CLK_UART1, 100 * 1000 * 1000);
+
 	iounmap(dpll_base);
 }
 
@@ -649,6 +653,9 @@ static void __init ath79_clocks_init_dt(
 	if (!clks[ATH79_CLK_MDIO])
 		clks[ATH79_CLK_MDIO] = clks[ATH79_CLK_REF];
 
+	if (!clks[ATH79_CLK_UART1])
+		clks[ATH79_CLK_UART1] = clks[ATH79_CLK_REF];
+
 	if (of_clk_add_provider(np, of_clk_src_onecell_get, &clk_data)) {
 		pr_err("%pOF: could not register clk provider\n", np);
 		goto err_iounmap;
--- a/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
+++ b/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
@@ -350,6 +350,7 @@
 #define AR934X_PLL_PCIE_CONFIG_PLL_PWD		BIT(30)
 
 #define AR934X_PLL_SWITCH_CLOCK_CONTROL_MDIO_CLK_SEL	BIT(6)
+#define AR934X_PLL_SWITCH_CLOCK_CONTROL_UART1_CLK_SEL	BIT(7)
 
 #define QCA953X_PLL_CPU_CONFIG_REG		0x00
 #define QCA953X_PLL_DDR_CONFIG_REG		0x04
--- a/include/dt-bindings/clock/ath79-clk.h
+++ b/include/dt-bindings/clock/ath79-clk.h
@@ -11,7 +11,8 @@
 #define ATH79_CLK_AHB		2
 #define ATH79_CLK_REF		3
 #define ATH79_CLK_MDIO		4
+#define ATH79_CLK_UART1		5
 
-#define ATH79_CLK_END		5
+#define ATH79_CLK_END		6
 
 #endif /* __DT_BINDINGS_ATH79_CLK_H */
