// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&pcie {
	status = "okay";

	ath10k: wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x0000 0 0 0 0>;

		nvmem-cells = <&calibration_ath10k>, <&macaddr_devdata_94 0>;
		nvmem-cell-names = "calibration", "mac-address";
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "bootloader";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "bdcfg";
				reg = <0x040000 0x010000>;

				bdcfg: nvmem-layout {
					compatible = "u-boot,env";
				};
			};

			partition@50000 {
				label = "devdata";
				reg = <0x050000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_devdata_94: macaddr@94 {
						compatible = "mac-base";
						reg = <0x94 0x11>;
						#nvmem-cell-cells = <1>;
					};

					macaddr_devdata_b0: macaddr@b0 {
						compatible = "mac-base";
						reg = <0xb0 0x11>;
						#nvmem-cell-cells = <1>;
					};
				};

			};

			partition@60000 {
				label = "devconf";
				reg = <0x060000 0x010000>;
				read-only;
			};

			partition@70000 {
				compatible = "seama";
				label = "firmware";
				reg = <0x070000 0xf80000>;
			};

			partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					calibration_ath9k: calibration@1000 {
						reg = <0x1000 0x440>;
					};

					calibration_ath10k: calibration@5000 {
						reg = <0x5000 0x844>;
					};
				};
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "sgmii";
		qca,mib-poll-interval = <500>;

		reset-gpios = <&gpio 11 GPIO_ACTIVE_LOW>;

		qca,ar8327-initvals = <
			0x04 0x00080080 /* PORT0 PAD MODE CTRL */
			0x10 0x81000080 /* POWER_ON_STRAP */
			0x50 0xcc35cc35 /* LED_CTRL0 */
			0x54 0xcb37cb37 /* LED_CTRL1 */
			0x58 0x00000000 /* LED_CTRL2 */
			0x5c 0x00f3cf00 /* LED_CTRL3 */
			0x7c 0x0000007e /* PORT0_STATUS */
			>;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x03000101 0x00000101 0x00001919>;

	phy-mode = "sgmii";
	phy-handle = <&phy0>;
};

&wmac {
	status = "okay";

	nvmem-cells = <&calibration_ath9k>, <&macaddr_devdata_b0 0>;
	nvmem-cell-names = "calibration", "mac-address";
};
