This add watchdog driver for broadcom 47xx device.
It uses the ssb subsytem to access embeded watchdog device.

Because the watchdog timeout is very short (about 2s), a soft timer is used
to increase the watchdog period.

Note : A patch for exporting the ssb_watchdog_timer_set will
be submitted on next linux-mips merge. Without this patch it can't 
be build as a module.

Signed-off-by: Aleksandar Radovanovic <biblbroks@sezampro.rs>
Signed-off-by: Matthieu CASTET <castet.matthieu@free.fr>
--- a/drivers/watchdog/Kconfig
+++ b/drivers/watchdog/Kconfig
@@ -764,6 +764,12 @@ config TXX9_WDT
 	help
 	  Hardware driver for the built-in watchdog timer on TXx9 MIPS SoCs.
 
+config BCM47XX_WDT
+	tristate "Broadcom BCM47xx Watchdog Timer"
+	depends on BCM47XX
+	help
+	  Hardware driver for the Broadcom BCM47xx Watchog Timer.
+
 # PARISC Architecture
 
 # POWERPC Architecture
--- a/drivers/watchdog/Makefile
+++ b/drivers/watchdog/Makefile
@@ -105,6 +105,7 @@ obj-$(CONFIG_WDT_RM9K_GPI) += rm9k_wdt.o
 obj-$(CONFIG_SIBYTE_WDOG) += sb_wdog.o
 obj-$(CONFIG_AR7_WDT) += ar7_wdt.o
 obj-$(CONFIG_TXX9_WDT) += txx9wdt.o
+obj-$(CONFIG_BCM47XX_WDT) += bcm47xx_wdt.o
 
 # PARISC Architecture
 
--- /dev/null
+++ b/drivers/watchdog/bcm47xx_wdt.c
@@ -0,0 +1,286 @@
+/*
+ *  Watchdog driver for Broadcom BCM47XX
+ *
+ *  Copyright (C) 2008 Aleksandar Radovanovic <biblbroks@sezampro.rs>
+ *  Copyright (C) 2009 Matthieu CASTET <castet.matthieu@free.fr>
+ *
+ *  This program is free software; you can redistribute it and/or
+ *  modify it under the terms of the GNU General Public License
+ *  as published by the Free Software Foundation; either version
+ *  2 of the License, or (at your option) any later version.
+ */
+
+#include <linux/bitops.h>
+#include <linux/errno.h>
+#include <linux/fs.h>
+#include <linux/init.h>
+#include <linux/kernel.h>
+#include <linux/miscdevice.h>
+#include <linux/module.h>
+#include <linux/moduleparam.h>
+#include <linux/reboot.h>
+#include <linux/types.h>
+#include <linux/uaccess.h>
+#include <linux/watchdog.h>
+#include <linux/timer.h>
+#include <linux/jiffies.h>
+#include <linux/ssb/ssb_embedded.h>
+#include <asm/mach-bcm47xx/bcm47xx.h>
+
+#define DRV_NAME		"bcm47xx_wdt"
+
+#define WDT_DEFAULT_TIME	30	/* seconds */
+#define WDT_MAX_TIME		256	/* seconds */
+
+static int wdt_time = WDT_DEFAULT_TIME;
+static int nowayout = WATCHDOG_NOWAYOUT;
+
+module_param(wdt_time, int, 0);
+MODULE_PARM_DESC(wdt_time, "Watchdog time in seconds. (default="
+				__MODULE_STRING(WDT_DEFAULT_TIME) ")");
+
+#ifdef CONFIG_WATCHDOG_NOWAYOUT
+module_param(nowayout, int, 0);
+MODULE_PARM_DESC(nowayout,
+		"Watchdog cannot be stopped once started (default="
+				__MODULE_STRING(WATCHDOG_NOWAYOUT) ")");
+#endif
+
+static unsigned long bcm47xx_wdt_busy;
+static char expect_release;
+static struct timer_list wdt_timer;
+static atomic_t ticks;
+
+static inline void bcm47xx_wdt_hw_start(void)
+{
+	/* this is 2,5s on 100Mhz clock  and 2s on 133 Mhz */
+	ssb_watchdog_timer_set(&ssb_bcm47xx, 0xfffffff);
+}
+
+static inline int bcm47xx_wdt_hw_stop(void)
+{
+	return ssb_watchdog_timer_set(&ssb_bcm47xx, 0);
+}
+
+static void bcm47xx_timer_tick(unsigned long unused)
+{
+	if (!atomic_dec_and_test(&ticks)) {
+		bcm47xx_wdt_hw_start();
+		mod_timer(&wdt_timer, jiffies + HZ);
+	} else {
+		printk(KERN_CRIT DRV_NAME "Watchdog will fire soon!!!\n");
+	}
+}
+
+static inline void bcm47xx_wdt_pet(void)
+{
+	atomic_set(&ticks, wdt_time);
+}
+
+static void bcm47xx_wdt_start(void)
+{
+	bcm47xx_wdt_pet();
+	bcm47xx_timer_tick(0);
+}
+
+static void bcm47xx_wdt_pause(void)
+{
+	del_timer_sync(&wdt_timer);
+	bcm47xx_wdt_hw_stop();
+}
+
+static void bcm47xx_wdt_stop(void)
+{
+	bcm47xx_wdt_pause();
+}
+
+static int bcm47xx_wdt_settimeout(int new_time)
+{
+	if ((new_time <= 0) || (new_time > WDT_MAX_TIME))
+		return -EINVAL;
+
+	wdt_time = new_time;
+	return 0;
+}
+
+static int bcm47xx_wdt_open(struct inode *inode, struct file *file)
+{
+	if (test_and_set_bit(0, &bcm47xx_wdt_busy))
+		return -EBUSY;
+
+	bcm47xx_wdt_start();
+	return nonseekable_open(inode, file);
+}
+
+static int bcm47xx_wdt_release(struct inode *inode, struct file *file)
+{
+	if (expect_release == 42) {
+		bcm47xx_wdt_stop();
+	} else {
+		printk(KERN_CRIT DRV_NAME
+			": Unexpected close, not stopping watchdog!\n");
+		bcm47xx_wdt_start();
+	}
+
+	clear_bit(0, &bcm47xx_wdt_busy);
+	expect_release = 0;
+	return 0;
+}
+
+static ssize_t bcm47xx_wdt_write(struct file *file, const char __user *data,
+			      size_t len, loff_t *ppos)
+{
+	if (len) {
+		if (!nowayout) {
+			size_t i;
+
+			expect_release = 0;
+
+			for (i = 0; i != len; i++) {
+				char c;
+				if (get_user(c, data + i))
+					return -EFAULT;
+				if (c == 'V')
+					expect_release = 42;
+			}
+		}
+		bcm47xx_wdt_pet();
+	}
+	return len;
+}
+
+static struct watchdog_info bcm47xx_wdt_info = {
+	.identity 	= DRV_NAME,
+	.options 	= WDIOF_SETTIMEOUT |
+				WDIOF_KEEPALIVEPING |
+				WDIOF_MAGICCLOSE,
+};
+
+static long bcm47xx_wdt_ioctl(struct file *file,
+					unsigned int cmd, unsigned long arg)
+{
+	void __user *argp = (void __user *)arg;
+	int __user *p = argp;
+	int new_value, retval = -EINVAL;;
+
+	switch (cmd) {
+	case WDIOC_GETSUPPORT:
+		return copy_to_user(argp, &bcm47xx_wdt_info,
+				sizeof(bcm47xx_wdt_info)) ? -EFAULT : 0;
+
+	case WDIOC_GETSTATUS:
+	case WDIOC_GETBOOTSTATUS:
+		return put_user(0, p);
+
+	case WDIOC_SETOPTIONS:
+		if (get_user(new_value, p))
+			return -EFAULT;
+
+		if (new_value & WDIOS_DISABLECARD) {
+			bcm47xx_wdt_stop();
+			retval = 0;
+		}
+
+		if (new_value & WDIOS_ENABLECARD) {
+			bcm47xx_wdt_start();
+			retval = 0;
+		}
+
+		return retval;
+
+	case WDIOC_KEEPALIVE:
+		bcm47xx_wdt_pet();
+		return 0;
+
+	case WDIOC_SETTIMEOUT:
+		if (get_user(new_value, p))
+			return -EFAULT;
+
+		if (bcm47xx_wdt_settimeout(new_value))
+			return -EINVAL;
+
+		bcm47xx_wdt_pet();
+
+	case WDIOC_GETTIMEOUT:
+		return put_user(wdt_time, p);
+
+	default:
+		return -ENOTTY;
+	}
+}
+
+static int bcm47xx_wdt_notify_sys(struct notifier_block *this,
+	   unsigned long code, void *unused)
+{
+	if (code == SYS_DOWN || code == SYS_HALT)
+		bcm47xx_wdt_stop();
+	return NOTIFY_DONE;
+}
+
+static const struct file_operations bcm47xx_wdt_fops = {
+	.owner		= THIS_MODULE,
+	.llseek		= no_llseek,
+	.unlocked_ioctl	= bcm47xx_wdt_ioctl,
+	.open		= bcm47xx_wdt_open,
+	.release	= bcm47xx_wdt_release,
+	.write		= bcm47xx_wdt_write,
+};
+
+static struct miscdevice bcm47xx_wdt_miscdev = {
+	.minor		= WATCHDOG_MINOR,
+	.name		= "watchdog",
+	.fops		= &bcm47xx_wdt_fops,
+};
+
+static struct notifier_block bcm47xx_wdt_notifier = {
+	.notifier_call = bcm47xx_wdt_notify_sys,
+};
+
+static int __init bcm47xx_wdt_init(void)
+{
+	int ret;
+
+	if (bcm47xx_wdt_hw_stop() < 0)
+		return -ENODEV;
+
+	setup_timer(&wdt_timer, bcm47xx_timer_tick, 0L);
+
+	if (bcm47xx_wdt_settimeout(wdt_time)) {
+		bcm47xx_wdt_settimeout(WDT_DEFAULT_TIME);
+		printk(KERN_INFO DRV_NAME
+			": wdt_time value must be 1 <= wdt_time <= 256, using %d\n",
+			wdt_time);
+	}
+
+	ret = register_reboot_notifier(&bcm47xx_wdt_notifier);
+	if (ret)
+		return ret;
+
+	ret = misc_register(&bcm47xx_wdt_miscdev);
+	if (ret) {
+		unregister_reboot_notifier(&bcm47xx_wdt_notifier);
+		return ret;
+	}
+
+	printk(KERN_INFO "BCM47xx Watchdog Timer enabled (%d seconds%s)\n",
+				wdt_time, nowayout ? ", nowayout" : "");
+	return 0;
+}
+
+static void __exit bcm47xx_wdt_exit(void)
+{
+	if (!nowayout)
+		bcm47xx_wdt_stop();
+
+	misc_deregister(&bcm47xx_wdt_miscdev);
+
+	unregister_reboot_notifier(&bcm47xx_wdt_notifier);
+}
+
+module_init(bcm47xx_wdt_init);
+module_exit(bcm47xx_wdt_exit);
+
+MODULE_AUTHOR("Aleksandar Radovanovic");
+MODULE_DESCRIPTION("Watchdog driver for Broadcom BCM47xx");
+MODULE_LICENSE("GPL");
+MODULE_ALIAS_MISCDEV(WATCHDOG_MINOR);
