--- a/arch/arm/mach-gemini/devices.c
+++ b/arch/arm/mach-gemini/devices.c
@@ -13,6 +13,7 @@
 #include <linux/platform_device.h>
 #include <linux/serial_8250.h>
 #include <linux/mtd/physmap.h>
+#include <linux/skbuff.h>
 
 #include <mach/irqs.h>
 #include <mach/hardware.h>
@@ -147,7 +148,7 @@ int platform_register_ethernet(struct ge
 	if (pdata->bus_id[1])
 		reg |= GMAC_1_ENABLE;
 	else if (pdata->interface[0] == PHY_INTERFACE_MODE_GMII)
-		reg |= GMAC_GMII;		
+		reg |= GMAC_GMII;
 
 	__raw_writel(reg, IO_ADDRESS(GEMINI_GLOBAL_BASE) + GLOBAL_MISC_CTRL);
 
--- a/drivers/net/phy/mdio-bitbang.c
+++ b/drivers/net/phy/mdio-bitbang.c
@@ -18,6 +18,7 @@
  */
 
 #include <linux/module.h>
+#include <linux/skbuff.h>
 #include <linux/mdio-bitbang.h>
 #include <linux/slab.h>
 #include <linux/types.h>
--- a/drivers/net/phy/mdio-gpio.c
+++ b/drivers/net/phy/mdio-gpio.c
@@ -25,6 +25,7 @@
 #include <linux/init.h>
 #include <linux/interrupt.h>
 #include <linux/platform_device.h>
+#include <linux/skbuff.h>
 #include <linux/gpio.h>
 #include <linux/mdio-gpio.h>
 
