From 146308ee673df13fafe40aaddc799e9ad58e6ecb Mon Sep 17 00:00:00 2001
From: Lars-Peter Clausen <lars@metafoo.de>
Date: Mon, 11 Jan 2010 04:29:42 +0100
Subject: [PATCH] /opt/Projects/openwrt/target/linux/xburst/patches-2.6.31/101-mmc.patch

---
 drivers/mmc/host/Kconfig  |    9 +++++++++
 drivers/mmc/host/Makefile |    1 +
 2 files changed, 10 insertions(+), 0 deletions(-)

--- a/drivers/mmc/host/Kconfig
+++ b/drivers/mmc/host/Kconfig
@@ -66,6 +66,15 @@ config MMC_RICOH_MMC
 	  useless. It is safe to select this driver even if you don't
 	  have a Ricoh based card reader.
 
+config MMC_JZ
+	tristate "JZ SD/Multimedia Card Interface support"
+	depends on SOC_JZ4720 || SOC_JZ4740
+	help
+	  This selects the Ingenic JZ4720/JZ4740 SD/Multimedia card Interface.
+	  If you have abIngenic platform with a Multimedia Card slot,
+	  say Y or M here.
+
+	  If unsure, say N.
 
 	  To compile this driver as a module, choose M here:
 	  the module will be called ricoh_mmc.
--- a/drivers/mmc/host/Makefile
+++ b/drivers/mmc/host/Makefile
@@ -6,6 +6,7 @@ ifeq ($(CONFIG_MMC_DEBUG),y)
 	EXTRA_CFLAGS		+= -DDEBUG
 endif
 
+obj-$(CONFIG_MMC_JZ)		+= jz_mmc.o
 obj-$(CONFIG_MMC_ARMMMCI)	+= mmci.o
 obj-$(CONFIG_MMC_PXA)		+= pxamci.o
 obj-$(CONFIG_MMC_IMX)		+= imxmmc.o
