--- /dev/null
+++ b/arch/arm/mach-gemini/board-wbd111.c
@@ -0,0 +1,125 @@
+/*
+ *  Support for Wiliboard WBD-111
+ *
+ *  Copyright (C) 2009 Imre Kaloz <kaloz@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ */
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/leds.h>
+#include <linux/input.h>
+#include <linux/skbuff.h>
+#include <linux/gpio_keys.h>
+#include <linux/mdio-gpio.h>
+#include <asm/mach-types.h>
+#include <asm/mach/arch.h>
+#include <asm/mach/time.h>
+
+#include <mach/gmac.h>
+
+#include "common.h"
+
+static struct mdio_gpio_platform_data wbd111_mdio = {
+	.mdc		= 22,
+	.mdio		= 21,
+	.phy_mask	= ~(1 << 1),
+};
+
+static struct platform_device wbd111_phy_device = {
+	.name	= "mdio-gpio",
+	.id	= 0,
+	.dev	= {
+		.platform_data = &wbd111_mdio,
+	},
+};
+
+static struct gemini_gmac_platform_data gmac_data = {
+	.bus_id[0] = "0:01",
+	.interface[0] = PHY_INTERFACE_MODE_MII,
+};
+
+static struct gpio_keys_button wbd111_keys[] = {
+	{
+		.code		= KEY_SETUP,
+		.gpio		= 5,
+		.active_low	= 1,
+		.desc		= "reset",
+		.type		= EV_KEY,
+	},
+};
+
+static struct gpio_keys_platform_data wbd111_keys_data = {
+	.buttons	= wbd111_keys,
+	.nbuttons	= ARRAY_SIZE(wbd111_keys),
+};
+
+static struct platform_device wbd111_keys_device = {
+	.name	= "gpio-keys",
+	.id	= -1,
+	.dev	= {
+		.platform_data = &wbd111_keys_data,
+	},
+};
+
+static struct gpio_led wbd111_leds[] = {
+	{
+		.name			= "L3red",
+		.gpio			= 1,
+	},
+	{
+		.name			= "L4green",
+		.gpio			= 2,
+	},
+	{
+		.name			= "L4red",
+		.gpio			= 3,
+	},
+	{
+		.name			= "L3green",
+		.gpio			= 5,
+	},
+};
+
+static struct gpio_led_platform_data wbd111_leds_data = {
+	.num_leds	= ARRAY_SIZE(wbd111_leds),
+	.leds		= wbd111_leds,
+};
+
+static struct platform_device wbd111_leds_device = {
+	.name	= "leds-gpio",
+	.id	= -1,
+	.dev	= {
+		.platform_data = &wbd111_leds_data,
+	},
+};
+
+static struct sys_timer wbd111_timer = {
+	.init	= gemini_timer_init,
+};
+
+static void __init wbd111_init(void)
+{
+	gemini_gpio_init();
+	platform_register_uart();
+	platform_register_watchdog();
+	platform_register_pflash(SZ_8M, NULL, 0);
+	platform_device_register(&wbd111_leds_device);
+	platform_device_register(&wbd111_keys_device);
+	platform_device_register(&wbd111_phy_device);
+	platform_register_ethernet(&gmac_data);
+}
+
+MACHINE_START(WBD111, "Wiliboard WBD-111")
+	.phys_io	= 0x7fffc000,
+	.io_pg_offst	= ((0xffffc000) >> 18) & 0xfffc,
+	.boot_params	= 0x100,
+	.map_io		= gemini_map_io,
+	.init_irq	= gemini_init_irq,
+	.timer		= &wbd111_timer,
+	.init_machine	= wbd111_init,
+MACHINE_END
--- a/arch/arm/mach-gemini/Kconfig
+++ b/arch/arm/mach-gemini/Kconfig
@@ -16,6 +16,13 @@ config MACH_RUT100
 	  Say Y here if you intend to run this kernel on a
 	  Teltonika 3G Router RUT100.
 
+config MACH_WBD111
+	bool "Wiliboard WBD-111"
+	select GEMINI_MEM_SWAP
+	help
+	  Say Y here if you intend to run this kernel on a
+	  Wiliboard WBD-111.
+
 endmenu
 
 config GEMINI_MEM_SWAP
--- a/arch/arm/mach-gemini/Makefile
+++ b/arch/arm/mach-gemini/Makefile
@@ -11,3 +11,4 @@ obj-$(CONFIG_PCI)	+= pci.o
 # Board-specific support
 obj-$(CONFIG_MACH_NAS4220B)	+= board-nas4220b.o
 obj-$(CONFIG_MACH_RUT100)	+= board-rut1xx.o
+obj-$(CONFIG_MACH_WBD111)	+= board-wbd111.o
