--- a/drivers/mtd/devices/at91_dataflash.c
+++ b/drivers/mtd/devices/at91_dataflash.c
@@ -175,7 +175,7 @@ static struct mtd_partition static_parti
 };
 #endif
 
-static const char *part_probes[] = { "cmdlinepart", NULL, };
+static const char *part_probes[] = { "cmdlinepart", "at91part", NULL, };
 
 #endif
 
--- a/drivers/mtd/Kconfig
+++ b/drivers/mtd/Kconfig
@@ -168,6 +168,12 @@ config MTD_OF_PARTS
 	  the partition map from the children of the flash node,
 	  as described in Documentation/powerpc/booting-without-of.txt.
 
+config MTD_AT91_PARTS
+	tristate "Atmel AT91 partitioning support"
+	depends on MTD_PARTITIONS && ARCH_AT91RM9200 && AT91_SPI
+	---help---
+	  Atmel AT91 partitioning support
+	
 comment "User Modules And Translation Layers"
 
 config MTD_CHAR
--- a/drivers/mtd/Makefile
+++ b/drivers/mtd/Makefile
@@ -12,6 +12,7 @@ obj-$(CONFIG_MTD_REDBOOT_PARTS) += redbo
 obj-$(CONFIG_MTD_CMDLINE_PARTS) += cmdlinepart.o
 obj-$(CONFIG_MTD_AFS_PARTS)	+= afs.o
 obj-$(CONFIG_MTD_OF_PARTS)      += ofpart.o
+obj-$(CONFIG_MTD_AT91_PARTS)   += at91part.o
 
 # 'Users' - code which presents functionality to userspace.
 obj-$(CONFIG_MTD_CHAR)		+= mtdchar.o
