From a3334c89fbed644bb12ee27e2d9c1dc70b1512ab Mon Sep 17 00:00:00 2001
From: Ivo van Doorn <IvDoorn@gmail.com>
Date: Sat, 14 Mar 2009 20:58:12 +0100
Subject: [PATCH] rt2x00: rt2x00: Move Move pci_dev specific access to rt2x00pci - part 2 (rt2800pci)

Signed-off-by: Ivo van Doorn <IvDoorn@gmail.com>
---
 drivers/net/wireless/rt2x00/rt2800pci.h |    6 ------
 1 files changed, 0 insertions(+), 6 deletions(-)

--- a/drivers/net/wireless/rt2x00/rt2800pci.h
+++ b/drivers/net/wireless/rt2x00/rt2800pci.h
@@ -83,12 +83,6 @@
  */
 
 /*
- * PCI Configuration Header
- */
-#define PCI_CONFIG_HEADER_VENDOR	0x0000
-#define PCI_CONFIG_HEADER_DEVICE	0x0002
-
-/*
  * E2PROM_CSR: EEPROM control register.
  * RELOAD: Write 1 to reload eeprom content.
  * TYPE: 0: 93c46, 1:93c66.
