--- a/drivers/rtc/rtc-ds1672.c
+++ b/drivers/rtc/rtc-ds1672.c
@@ -13,10 +13,10 @@
 #include <linux/i2c.h>
 #include <linux/rtc.h>
 
-#define DRV_VERSION "0.3"
+#define DRV_VERSION "0.4"
 
-/* Addresses to scan: none. This chip cannot be detected. */
-static unsigned short normal_i2c[] = { I2C_CLIENT_END };
+/* Addresses to scan: 0x68 */
+static unsigned short normal_i2c[] = { 0x68, I2C_CLIENT_END };
 
 /* Insmod parameters */
 I2C_CLIENT_INSMOD;
