From be378ebd6cfb8e369d4aa03a551e594d00debda5 Mon Sep 17 00:00:00 2001
From: Sky Huang <skylake.huang@mediatek.com>
Date: Thu, 13 Feb 2025 16:05:53 +0800
Subject: [PATCH 5/5] net: phy: mediatek: Move some macros to phy-lib for later
 use

Move some macros to phy-lib because MediaTek's 2.5G built-in
ethernet PHY will also use them.

Signed-off-by: Sky Huang <skylake.huang@mediatek.com>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Link: https://patch.msgid.link/20250213080553.921434-6-SkyLake.Huang@mediatek.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/phy/mediatek/mtk-ge.c | 4 ----
 drivers/net/phy/mediatek/mtk.h    | 4 ++++
 2 files changed, 4 insertions(+), 4 deletions(-)

--- a/drivers/net/phy/mediatek/mtk-ge.c
+++ b/drivers/net/phy/mediatek/mtk-ge.c
@@ -8,10 +8,6 @@
 #define MTK_GPHY_ID_MT7530		0x03a29412
 #define MTK_GPHY_ID_MT7531		0x03a29441
 
-#define MTK_PHY_PAGE_EXTENDED_1			0x0001
-#define MTK_PHY_AUX_CTRL_AND_STATUS		0x14
-#define   MTK_PHY_ENABLE_DOWNSHIFT		BIT(4)
-
 #define MTK_PHY_PAGE_EXTENDED_2			0x0002
 #define MTK_PHY_PAGE_EXTENDED_3			0x0003
 #define MTK_PHY_RG_LPI_PCS_DSP_CTRL_REG11	0x11
--- a/drivers/net/phy/mediatek/mtk.h
+++ b/drivers/net/phy/mediatek/mtk.h
@@ -8,7 +8,11 @@
 #ifndef _MTK_EPHY_H_
 #define _MTK_EPHY_H_
 
+#define MTK_PHY_AUX_CTRL_AND_STATUS		0x14
+#define   MTK_PHY_ENABLE_DOWNSHIFT		BIT(4)
+
 #define MTK_EXT_PAGE_ACCESS			0x1f
+#define MTK_PHY_PAGE_EXTENDED_1			0x0001
 #define MTK_PHY_PAGE_STANDARD			0x0000
 #define MTK_PHY_PAGE_EXTENDED_52B5		0x52b5
 
