From 219cecbb3e864685a1f08bcb79ce07d9bc4f506e Mon Sep 17 00:00:00 2001
From: "SkyLake.Huang" <skylake.huang@mediatek.com>
Date: Sat, 9 Nov 2024 00:34:55 +0800
Subject: [PATCH] net: phy: mediatek: add MT7530 & MT7531's PHY ID macros

This patch adds MT7530 & MT7531's PHY ID macros in mtk-ge.c so that
it follows the same rule of mtk-ge-soc.c.

Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: SkyLake.Huang <skylake.huang@mediatek.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/phy/mediatek/mtk-ge.c | 11 +++++++----
 1 file changed, 7 insertions(+), 4 deletions(-)

--- a/drivers/net/phy/mediatek/mtk-ge.c
+++ b/drivers/net/phy/mediatek/mtk-ge.c
@@ -5,6 +5,9 @@
 
 #include "mtk.h"
 
+#define MTK_GPHY_ID_MT7530		0x03a29412
+#define MTK_GPHY_ID_MT7531		0x03a29441
+
 #define MTK_EXT_PAGE_ACCESS		0x1f
 #define MTK_PHY_PAGE_STANDARD		0x0000
 #define MTK_PHY_PAGE_EXTENDED		0x0001
@@ -62,7 +65,7 @@ static int mt7531_phy_config_init(struct
 
 static struct phy_driver mtk_gephy_driver[] = {
 	{
-		PHY_ID_MATCH_EXACT(0x03a29412),
+		PHY_ID_MATCH_EXACT(MTK_GPHY_ID_MT7530),
 		.name		= "MediaTek MT7530 PHY",
 		.config_init	= mt7530_phy_config_init,
 		/* Interrupts are handled by the switch, not the PHY
@@ -76,7 +79,7 @@ static struct phy_driver mtk_gephy_drive
 		.write_page	= mtk_phy_write_page,
 	},
 	{
-		PHY_ID_MATCH_EXACT(0x03a29441),
+		PHY_ID_MATCH_EXACT(MTK_GPHY_ID_MT7531),
 		.name		= "MediaTek MT7531 PHY",
 		.config_init	= mt7531_phy_config_init,
 		/* Interrupts are handled by the switch, not the PHY
@@ -94,8 +97,8 @@ static struct phy_driver mtk_gephy_drive
 module_phy_driver(mtk_gephy_driver);
 
 static struct mdio_device_id __maybe_unused mtk_gephy_tbl[] = {
-	{ PHY_ID_MATCH_EXACT(0x03a29441) },
-	{ PHY_ID_MATCH_EXACT(0x03a29412) },
+	{ PHY_ID_MATCH_EXACT(MTK_GPHY_ID_MT7530) },
+	{ PHY_ID_MATCH_EXACT(MTK_GPHY_ID_MT7531) },
 	{ }
 };
 
