(kicad_symbol_lib (version 20211014) (generator entropy_generator)
  (symbol "TAC5112IRGER" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 29.21 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "TAC5112IRGER" (at 29.21 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "TAC5112IRGER" (at 29.21 -94.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tac5112.pdf?ts=1748263003675&ref_url=https%253A%252F%252Fwww.ti.com%252Fde-de%252Faudio-ic%252Fconverters%252Fproducts.html" (at 29.21 -194.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "Interface - CODECs Low-power stereo audio codec with 105dB dynamic range ADC and 114dB dynamic range DAC, -40C ~ 125C, 1.2V/3.3V" (at 29.21 -294.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "1" (at 29.21 -394.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "" (at 29.21 -494.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "" (at 29.21 -594.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "Texas Instruments" (at 29.21 -694.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "TAC5112IRGER" (at 29.21 -794.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 2.54)
      (end 27.94 -38.1)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "DREG" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "BCLK" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "FSYNC" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "DOUT" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -10.16 0) (length 5.08)
      (name "DIN" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -12.7 0) (length 5.08)
      (name "IOVDD" (effects (font (size 1.27 1.27))))
      (number "6" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -15.24 0) (length 5.08)
      (name "SCL" (effects (font (size 1.27 1.27))))
      (number "7" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -17.78 0) (length 5.08)
      (name "SDA" (effects (font (size 1.27 1.27))))
      (number "8" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -20.32 0) (length 5.08)
      (name "GPIO1" (effects (font (size 1.27 1.27))))
      (number "9" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -22.86 0) (length 5.08)
      (name "GPIO2" (effects (font (size 1.27 1.27))))
      (number "10" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -25.4 0) (length 5.08)
      (name "GPO1" (effects (font (size 1.27 1.27))))
      (number "11" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -27.94 0) (length 5.08)
      (name "GPI1" (effects (font (size 1.27 1.27))))
      (number "12" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -30.48 0) (length 5.08)
      (name "ADDR" (effects (font (size 1.27 1.27))))
      (number "13" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -33.02 0) (length 5.08)
      (name "MICBIAS" (effects (font (size 1.27 1.27))))
      (number "14" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -35.56 0) (length 5.08)
      (name "IN1P" (effects (font (size 1.27 1.27))))
      (number "15" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 0 180) (length 5.08)
      (name "IN1M" (effects (font (size 1.27 1.27))))
      (number "16" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -2.54 180) (length 5.08)
      (name "IN2P" (effects (font (size 1.27 1.27))))
      (number "17" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -5.08 180) (length 5.08)
      (name "IN2M" (effects (font (size 1.27 1.27))))
      (number "18" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -7.62 180) (length 5.08)
      (name "OUT1M" (effects (font (size 1.27 1.27))))
      (number "19" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -10.16 180) (length 5.08)
      (name "OUT1P" (effects (font (size 1.27 1.27))))
      (number "20" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -12.7 180) (length 5.08)
      (name "OUT2P" (effects (font (size 1.27 1.27))))
      (number "21" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -15.24 180) (length 5.08)
      (name "OUT2M" (effects (font (size 1.27 1.27))))
      (number "22" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -17.78 180) (length 5.08)
      (name "AVDD" (effects (font (size 1.27 1.27))))
      (number "23" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -20.32 180) (length 5.08)
      (name "VREF" (effects (font (size 1.27 1.27))))
      (number "24" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -22.86 180) (length 5.08)
      (name "VSS_1" (effects (font (size 1.27 1.27))))
      (number "25" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -25.4 180) (length 5.08)
      (name "VSS_2" (effects (font (size 1.27 1.27))))
      (number "26" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -27.94 180) (length 5.08)
      (name "VSS_3" (effects (font (size 1.27 1.27))))
      (number "27" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -30.48 180) (length 5.08)
      (name "VSS_4" (effects (font (size 1.27 1.27))))
      (number "28" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -33.02 180) (length 5.08)
      (name "VSS_5" (effects (font (size 1.27 1.27))))
      (number "29" (effects (font (size 1.27 1.27))))
    )
  )
)
