(footprint "QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "QFN, 16 Pin (https://www.st.com/resource/en/datasheet/tsv521.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -2.83 0)
		(layer "F.SilkS")
		(uuid "146cb097-3a23-4d30-97e1-02afe1715ff0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm_ThermalVias"
		(at 0 2.83 0)
		(layer "F.Fab")
		(uuid "d51956ff-1267-4fa4-aec0-e779bb076052")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "e2650296-9dce-4213-b9ad-c5957d95e9de")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "6e80eac6-0820-4ed8-a62e-21d57212afde")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.61 -1.135)
		(end -1.61 -1.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "794740e0-cbde-4527-bb22-0b4a4c74449a")
	)
	(fp_line
		(start -1.61 1.61)
		(end -1.61 1.135)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c30118cb-93db-4f00-bbdd-7910b11869d7")
	)
	(fp_line
		(start -1.135 -1.61)
		(end -1.31 -1.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "56f5158c-dd8a-4f6b-a21f-5dd799b5c1d5")
	)
	(fp_line
		(start -1.135 1.61)
		(end -1.61 1.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f2ff359a-2256-4cd4-9da3-a5271d0a8189")
	)
	(fp_line
		(start 1.135 -1.61)
		(end 1.61 -1.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c1dcc67e-52ae-449e-9108-f8c4480d93b1")
	)
	(fp_line
		(start 1.135 1.61)
		(end 1.61 1.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4cdce9dd-a812-4039-8e65-2ae3cd56f9df")
	)
	(fp_line
		(start 1.61 -1.61)
		(end 1.61 -1.135)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "162babcd-8007-46c5-80bd-bbd89b0f6948")
	)
	(fp_line
		(start 1.61 1.61)
		(end 1.61 1.135)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "65658de6-bfbe-46ba-95a4-533601177c79")
	)
	(fp_poly
		(pts
			(xy -1.61 -1.61) (xy -1.85 -1.94) (xy -1.37 -1.94)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "5056cf90-be6a-434a-a325-4a362c32af51")
	)
	(fp_line
		(start -2.13 -1.13)
		(end -1.75 -1.13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1f671b79-d97e-41ad-93fc-1cf51bfa9cb7")
	)
	(fp_line
		(start -2.13 1.13)
		(end -2.13 -1.13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a08deeeb-cd7c-4232-a316-3dafdfdfd22c")
	)
	(fp_line
		(start -1.75 -1.75)
		(end -1.13 -1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "662e0b38-7053-4314-a76b-084e7c6272ce")
	)
	(fp_line
		(start -1.75 -1.13)
		(end -1.75 -1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d0e2a759-83b1-40db-b43d-005c3d7d23ae")
	)
	(fp_line
		(start -1.75 1.13)
		(end -2.13 1.13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "19883e16-6c0d-436f-ba5b-4a05292297c2")
	)
	(fp_line
		(start -1.75 1.75)
		(end -1.75 1.13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "186bab08-2bad-43d1-8f48-d50ecde883cb")
	)
	(fp_line
		(start -1.13 -2.13)
		(end 1.13 -2.13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "64b466da-5271-4218-b766-7f4aa5c20160")
	)
	(fp_line
		(start -1.13 -1.75)
		(end -1.13 -2.13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f05331ee-774e-4698-b4c8-3d8e70d9b824")
	)
	(fp_line
		(start -1.13 1.75)
		(end -1.75 1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fabffa53-ad6d-493c-8f94-421324445e39")
	)
	(fp_line
		(start -1.13 2.13)
		(end -1.13 1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a496d30d-77fa-498c-ad3a-d5a1f0bdb36e")
	)
	(fp_line
		(start 1.13 -2.13)
		(end 1.13 -1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "eedb0013-7f64-4e9b-8709-ac33ef35ba86")
	)
	(fp_line
		(start 1.13 -1.75)
		(end 1.75 -1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6965b92e-f026-4522-b39c-d1a84a46ed6f")
	)
	(fp_line
		(start 1.13 1.75)
		(end 1.13 2.13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b8956d33-1761-4836-a804-bbf2b778e549")
	)
	(fp_line
		(start 1.13 2.13)
		(end -1.13 2.13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3627ec72-7ac6-4784-8218-dad7d4bfa806")
	)
	(fp_line
		(start 1.75 -1.75)
		(end 1.75 -1.13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ec936198-d501-46f6-a690-abfa32a3b8cb")
	)
	(fp_line
		(start 1.75 -1.13)
		(end 2.13 -1.13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f219ea12-929d-42d5-98d3-50eb61c80fbc")
	)
	(fp_line
		(start 1.75 1.13)
		(end 1.75 1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f7a71f8d-a99f-4e39-9862-af6ac30a7091")
	)
	(fp_line
		(start 1.75 1.75)
		(end 1.13 1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "817093f7-d70e-4e8d-a938-0d501369996e")
	)
	(fp_line
		(start 2.13 -1.13)
		(end 2.13 1.13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "db88c6f6-4b31-4243-9654-30d77b022a33")
	)
	(fp_line
		(start 2.13 1.13)
		(end 1.75 1.13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "393772b7-f5af-49e8-9612-4b8bb9d9a9ba")
	)
	(fp_poly
		(pts
			(xy -1.5 -0.75) (xy -1.5 1.5) (xy 1.5 1.5) (xy 1.5 -1.5) (xy -0.75 -1.5)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "c0565ff4-e04c-4de1-8a69-8b14d4a59ec7")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "69b96c44-6392-4f22-8818-ebb39567f873")
		(effects
			(font
				(size 0.75 0.75)
				(thickness 0.11)
			)
		)
	)
	(pad "" smd roundrect
		(at -0.425 -0.425)
		(size 0.69 0.69)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "edb080ec-f862-442f-a07c-f3f822e92eac")
	)
	(pad "" smd roundrect
		(at -0.425 0.425)
		(size 0.69 0.69)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "400bcf57-b44e-4c5a-ab46-c04b3cab419b")
	)
	(pad "" smd roundrect
		(at 0.425 -0.425)
		(size 0.69 0.69)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "f168171f-5a00-478e-a94a-74957d998f5a")
	)
	(pad "" smd roundrect
		(at 0.425 0.425)
		(size 0.69 0.69)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "a70fb6f2-aa93-4fbd-992d-d2143f65e9aa")
	)
	(pad "1" smd roundrect
		(at -1.4625 -0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "f263de75-8f03-4c0d-bbe8-69115199632e")
	)
	(pad "2" smd roundrect
		(at -1.4625 -0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "26b64c03-186c-4209-b768-66b3958013f9")
	)
	(pad "3" smd roundrect
		(at -1.4625 0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "ad332282-e7de-46d5-8d74-4a20c5bb6abc")
	)
	(pad "4" smd roundrect
		(at -1.4625 0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "90175b93-a479-4dd8-9b85-6c77b02a9199")
	)
	(pad "5" smd roundrect
		(at -0.75 1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "38674765-a05d-46f1-becd-9c3168ad661a")
	)
	(pad "6" smd roundrect
		(at -0.25 1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "ce7f813e-4f7e-4157-84af-b30a379f3210")
	)
	(pad "7" smd roundrect
		(at 0.25 1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "eca66c6d-1ffa-440b-bffa-bb087cb75123")
	)
	(pad "8" smd roundrect
		(at 0.75 1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "b38d6cac-61a7-46a7-8872-2596081f1ce3")
	)
	(pad "9" smd roundrect
		(at 1.4625 0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "54ab9335-8987-4f76-bf90-b5d0da4be022")
	)
	(pad "10" smd roundrect
		(at 1.4625 0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "3fea1b13-3ae4-44a1-83d0-6b9b84e406bf")
	)
	(pad "11" smd roundrect
		(at 1.4625 -0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "0bef8fe5-c2dc-4b06-a1ae-68ad9d8423f4")
	)
	(pad "12" smd roundrect
		(at 1.4625 -0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "f1f5f2fb-694f-4fdf-ba18-2a55ecdb8b77")
	)
	(pad "13" smd roundrect
		(at 0.75 -1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "70c63b74-ad50-4cf2-b27a-daad0df06ca2")
	)
	(pad "14" smd roundrect
		(at 0.25 -1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "9014df83-ce34-4861-b73d-5f0081a34d0f")
	)
	(pad "15" smd roundrect
		(at -0.25 -1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "a796753a-1977-4937-9ac1-45fdde894bba")
	)
	(pad "16" smd roundrect
		(at -0.75 -1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "f13fdf09-8954-47b4-95d7-5f517ea93f7d")
	)
	(pad "17" thru_hole circle
		(at -0.55 -0.55)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "2cf49eb3-69ae-489c-a1a9-fd78a76faff6")
	)
	(pad "17" thru_hole circle
		(at -0.55 0)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "940fd9f5-bc60-4156-84bd-47db1f493b07")
	)
	(pad "17" thru_hole circle
		(at -0.55 0.55)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "fc118f21-1667-4e35-b534-3bfbff79aab8")
	)
	(pad "17" thru_hole circle
		(at 0 -0.55)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "c12a4c25-d958-4e3f-b071-1f45f1378f36")
	)
	(pad "17" thru_hole circle
		(at 0 0)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "23510b70-47cb-4362-8a39-9db1315f4f7a")
	)
	(pad "17" smd roundrect
		(at 0 0)
		(size 1.7 1.7)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.05882352941)
		(zone_connect 2)
		(uuid "4eaa4886-87a8-421e-9a38-c05f26a21d1f")
	)
	(pad "17" smd roundrect
		(at 0 0)
		(size 1.7 1.7)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(roundrect_rratio 0.05882352941)
		(zone_connect 2)
		(uuid "e511c39e-f8fb-42ad-a37a-e49d7bebf859")
	)
	(pad "17" thru_hole circle
		(at 0 0.55)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "45eeca99-2c2c-4d89-8529-b816a2dec996")
	)
	(pad "17" thru_hole circle
		(at 0.55 -0.55)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "ec8d14d2-db2f-48d9-a4aa-73b79c5ec504")
	)
	(pad "17" thru_hole circle
		(at 0.55 0)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "74e6a742-89cf-4343-bff9-14ed4f09e303")
	)
	(pad "17" thru_hole circle
		(at 0.55 0.55)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "484c7ef4-0746-459d-a501-e944bc0a4d11")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
