(footprint "Connector_FFC_01x20_P0.75mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Display connector with 0.75 mm pitch and 0.5 mm pads.")
	(property "Reference" "REF**"
		(at 1.1 -16.8 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "96da1233-e675-4c8c-afaf-4475eb5d9824")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Connector_FFC_01x20_P0.75mm"
		(at 0 2.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "554649ae-ab4f-406a-badd-db07580cff87")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "74ce53c0-553a-49b8-ac0a-254203f1eb13")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1458e767-c4d0-4651-b4d6-a101cb8adef0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -0.8 -16.1)
		(end -0.8 -14.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c7155c5b-2c74-460a-9f4a-0796184565a4")
	)
	(fp_line
		(start -0.8 0.4)
		(end -0.8 1.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "604821a7-773a-40c5-8f67-bfa9b866f9a8")
	)
	(fp_line
		(start -0.6 0.6)
		(end -0.4 0.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "90c5d88c-4fd8-40b6-aada-e089d72e4acf")
	)
	(fp_line
		(start -0.6 1.6)
		(end -0.6 0.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "196a5370-2581-46cc-abb1-0729cbd31024")
	)
	(fp_line
		(start 0 -16.1)
		(end -0.8 -16.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "79abb49b-8440-4723-a83d-fd1153da9c99")
	)
	(fp_line
		(start 0 1.9)
		(end -0.8 1.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1d0fb3f6-db61-49e3-bc36-704571460dfe")
	)
	(fp_line
		(start 0.8 1.9)
		(end 3.9 1.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ab8dc371-4855-4d09-9602-5a59d9c91676")
	)
	(fp_line
		(start 3.9 -16.1)
		(end 0.8 -16.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b5e3023f-b5f8-42ce-86a8-2efba519cf08")
	)
	(fp_line
		(start 4.4 1.400001)
		(end 4.4 -15.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "4d28bb08-642a-4522-95a8-803670063fe2")
	)
	(fp_arc
		(start 0 1.9)
		(mid 0.4 1.5)
		(end 0.8 1.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "562e0a0e-d44e-4a05-a218-c3830e5b2505")
	)
	(fp_arc
		(start 0.8 -16.1)
		(mid 0.4 -15.7)
		(end 0 -16.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c0803e84-3c77-4944-bf09-6b29910b55bd")
	)
	(fp_arc
		(start 3.9 -16.1)
		(mid 4.253553 -15.953553)
		(end 4.4 -15.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d7727b99-9d03-49d6-b942-2fd619393ef1")
	)
	(fp_arc
		(start 4.400001 1.400001)
		(mid 4.253554 1.753554)
		(end 3.900001 1.900001)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ebce25d4-aff1-41e0-9ce3-0e25b85c01fc")
	)
	(fp_text user "${REFERENCE}"
		(at 2.8 -7.2 90)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b143fb04-31a7-4b1e-9b3b-5aa9cac39fc0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at 0 0)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "d17a798a-037b-43a8-afc0-412877154d0f")
	)
	(pad "2" smd roundrect
		(at 0 -0.75)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "a24f85ea-ff8c-4756-861a-fd662096b124")
	)
	(pad "3" smd roundrect
		(at 0 -1.5)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "e029bf28-0402-488c-a365-88640e3b1cc3")
	)
	(pad "4" smd roundrect
		(at 0 -2.25)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "bee3b2b6-c686-46ff-a660-c6c408f2b025")
	)
	(pad "5" smd roundrect
		(at 0 -3)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "1c5c81e0-37fa-4601-822f-135e50813e58")
	)
	(pad "6" smd roundrect
		(at 0 -3.75)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "6e60ff3d-3007-4bfc-a8d7-1b3fba17fab7")
	)
	(pad "7" smd roundrect
		(at 0 -4.5)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "a6a23fbb-1a12-4e27-a23c-3f0832f3dcf5")
	)
	(pad "8" smd roundrect
		(at 0 -5.25)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "423c104d-1379-4108-8e0a-7245b0db38c7")
	)
	(pad "9" smd roundrect
		(at 0 -6)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "b01a38bb-388f-4010-b706-0bef5f06f89a")
	)
	(pad "10" smd roundrect
		(at 0 -6.75)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "7248bf28-9550-4ce5-93ff-b1ced1217e5c")
	)
	(pad "11" smd roundrect
		(at 0 -7.5)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "467fb758-d94e-4c73-802b-422d396ae577")
	)
	(pad "12" smd roundrect
		(at 0 -8.25)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "06c8a2db-4d9f-49a4-8753-4c2ea1a5a8ca")
	)
	(pad "13" smd roundrect
		(at 0 -9)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "06f25f55-a767-4020-8a64-fe4d9e6edf32")
	)
	(pad "14" smd roundrect
		(at 0 -9.75)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "f630ac7e-07fc-4286-9ff7-c24c15f12f71")
	)
	(pad "15" smd roundrect
		(at 0 -10.5)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "2968b8c7-b308-4711-be23-f4e260c8d146")
	)
	(pad "16" smd roundrect
		(at 0 -11.25)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "56f8d723-adc8-40a7-a6de-707705b327f4")
	)
	(pad "17" smd roundrect
		(at 0 -12)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "e0db5e44-f434-4323-9404-5c7e3f77af52")
	)
	(pad "18" smd roundrect
		(at 0 -12.75)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "ebcfb2ca-8559-45b6-809f-b74e7398c6d3")
	)
	(pad "19" smd roundrect
		(at 0 -13.5)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "ad691881-1d54-4ee5-845a-fecd66ef2fff")
	)
	(pad "20" smd roundrect
		(at 0 -14.25)
		(size 2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
		(uuid "f04e77fa-ddee-4f03-861e-42d55e063fd1")
	)
	(embedded_fonts no)
)
