(kicad_symbol_lib (version 20211014) (generator entropy_generator)
  (symbol "SX1255IWLTRT" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 31.75 20.32 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "SX1255IWLTRT" (at 31.75 17.78 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "QFN50P500X500X80-33N-D" (at 31.75 -82.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://datasheet.datasheetarchive.com/originals/distributors/DKDS-5/90665.pdf" (at 31.75 -182.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "RF Transceiver RF Front End Transceiver" (at 31.75 -282.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "0.8" (at 31.75 -382.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "947-SX1255IWLTRT" (at 31.75 -482.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Semtech/SX1255IWLTRT?qs=rBWM4%252BvDhIdl5dK4JoeveQ%3D%3D" (at 31.75 -582.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "SEMTECH" (at 31.75 -682.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "SX1255IWLTRT" (at 31.75 -782.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 15.24)
      (end 30.48 -30.48)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "VR_PA" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "VBATI" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "VR_ANAI" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "GND_1" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -10.16 0) (length 5.08)
      (name "VR_DIG" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -12.7 0) (length 5.08)
      (name "XTA" (effects (font (size 1.27 1.27))))
      (number "6" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -15.24 0) (length 5.08)
      (name "GND_2" (effects (font (size 1.27 1.27))))
      (number "7" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -17.78 0) (length 5.08)
      (name "XTB" (effects (font (size 1.27 1.27))))
      (number "8" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 7.62 -35.56 90) (length 5.08)
      (name "RESET" (effects (font (size 1.27 1.27))))
      (number "9" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 10.16 -35.56 90) (length 5.08)
      (name "CK_OUT" (effects (font (size 1.27 1.27))))
      (number "10" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 12.7 -35.56 90) (length 5.08)
      (name "CK_IN" (effects (font (size 1.27 1.27))))
      (number "11" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 15.24 -35.56 90) (length 5.08)
      (name "Q_IN" (effects (font (size 1.27 1.27))))
      (number "12" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 17.78 -35.56 90) (length 5.08)
      (name "I_IN" (effects (font (size 1.27 1.27))))
      (number "13" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 20.32 -35.56 90) (length 5.08)
      (name "Q_OUT" (effects (font (size 1.27 1.27))))
      (number "14" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 22.86 -35.56 90) (length 5.08)
      (name "I_OUT" (effects (font (size 1.27 1.27))))
      (number "15" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 25.4 -35.56 90) (length 5.08)
      (name "VBAT2" (effects (font (size 1.27 1.27))))
      (number "16" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 0 180) (length 5.08)
      (name "DIO3" (effects (font (size 1.27 1.27))))
      (number "24" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -2.54 180) (length 5.08)
      (name "DIO2" (effects (font (size 1.27 1.27))))
      (number "23" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -5.08 180) (length 5.08)
      (name "DIO1" (effects (font (size 1.27 1.27))))
      (number "22" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -7.62 180) (length 5.08)
      (name "DIO0" (effects (font (size 1.27 1.27))))
      (number "21" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -10.16 180) (length 5.08)
      (name "NSS" (effects (font (size 1.27 1.27))))
      (number "20" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -12.7 180) (length 5.08)
      (name "MOSI" (effects (font (size 1.27 1.27))))
      (number "19" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -15.24 180) (length 5.08)
      (name "MISO" (effects (font (size 1.27 1.27))))
      (number "18" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -17.78 180) (length 5.08)
      (name "SCK" (effects (font (size 1.27 1.27))))
      (number "17" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 7.62 20.32 270) (length 5.08)
      (name "GND_6" (effects (font (size 1.27 1.27))))
      (number "33" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 10.16 20.32 270) (length 5.08)
      (name "VBAT3" (effects (font (size 1.27 1.27))))
      (number "32" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 12.7 20.32 270) (length 5.08)
      (name "GND_5" (effects (font (size 1.27 1.27))))
      (number "31" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 15.24 20.32 270) (length 5.08)
      (name "RFO_P" (effects (font (size 1.27 1.27))))
      (number "30" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 17.78 20.32 270) (length 5.08)
      (name "RFO_N" (effects (font (size 1.27 1.27))))
      (number "29" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 20.32 20.32 270) (length 5.08)
      (name "GND_4" (effects (font (size 1.27 1.27))))
      (number "28" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 22.86 20.32 270) (length 5.08)
      (name "RFI" (effects (font (size 1.27 1.27))))
      (number "27" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 25.4 20.32 270) (length 5.08)
      (name "GND_3" (effects (font (size 1.27 1.27))))
      (number "26" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 27.94 20.32 270) (length 5.08)
      (name "VR_ANA2" (effects (font (size 1.27 1.27))))
      (number "25" (effects (font (size 1.27 1.27))))
    )
  )
)
