(footprint "Jack_3.5mm_CUI_SJ1-3525N_Modified"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
	(tags "TRS audio jack stereo horizontal")
	(property "Reference" "REF**"
		(at 0 -8.8 0)
		(layer "F.SilkS")
		(uuid "1add7dcf-a760-4acf-a8df-7191842316d8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Jack_3.5mm_CUI_SJ1-3525N_Modified"
		(at 0 -10 0)
		(layer "F.Fab")
		(uuid "6612f225-863e-4980-926d-c81f7a4c0ba5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "87b43f88-e722-4fe0-a9f0-7872afe98c67")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fcc3ef8c-8425-4c05-ab28-aa0bbbe4a25a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -6 -7.7)
		(end 6 -7.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c4ed921b-5978-4907-b8ae-6b0640f1dea6")
	)
	(fp_line
		(start -6 3.3)
		(end -6 -7.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "11374064-f99a-4833-9a35-64656a6379df")
	)
	(fp_line
		(start -4.5 3.3)
		(end -6 3.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fcc64e02-2983-4a1e-a31b-27dcbbb26eb0")
	)
	(fp_line
		(start -4.5 4.5)
		(end -4.5 3.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5973c661-5067-4d11-9c7c-eb9ecb3fcf1e")
	)
	(fp_line
		(start -3 4.5)
		(end -4.5 4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5f44e682-5a0e-4909-91c5-de6e1fd3e758")
	)
	(fp_line
		(start -3 6.3)
		(end -3 4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "12804b3f-e88a-4b05-8f3f-5e0cea0160bf")
	)
	(fp_line
		(start -2 3.3)
		(end -2 6.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fe268b09-68ad-41a9-be41-1a6da3eae22d")
	)
	(fp_line
		(start 2 3.3)
		(end -2 3.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d6f8847e-63f1-4d60-b6d0-26b3d97acaf0")
	)
	(fp_line
		(start 2 6.3)
		(end 2 3.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b6f51c18-3efd-4627-a77f-6d7cc1dccb64")
	)
	(fp_line
		(start 3 4.5)
		(end 3 6.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d0f77083-129b-4203-807d-640854c1c549")
	)
	(fp_line
		(start 3 6.3)
		(end -3 6.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2f7a40ad-250c-4f5a-8245-765c568de5c7")
	)
	(fp_line
		(start 4.5 3.3)
		(end 4.5 4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "17b9415d-4048-4dad-a12f-0690dcdf82b5")
	)
	(fp_line
		(start 4.5 4.5)
		(end 3 4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dfb46782-e4ff-42a6-8adb-edd75045139d")
	)
	(fp_line
		(start 6 -7.7)
		(end 6 3.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dcf98f86-aaf6-490c-98c3-b153f5552ef1")
	)
	(fp_line
		(start 6 3.3)
		(end 4.5 3.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ad62fed3-471e-4fc4-a7a0-4482ab1ce7ee")
	)
	(fp_line
		(start -3.15 3.500002)
		(end -3.15 5.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "48f41604-a6e1-4446-881f-772a3ab9e3cf")
	)
	(fp_line
		(start -3.15 5.35)
		(end -6 5.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "910d111c-8356-4b3a-a4cd-22f14c2881a3")
	)
	(fp_line
		(start 2.75 3.1)
		(end -2.75 3.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "5a978aba-42e4-4034-9a73-91bf03f2f54d")
	)
	(fp_line
		(start 3.15 3.5)
		(end 3.15 5.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "cef4abab-1d99-4638-bfd7-bf65ee264ed6")
	)
	(fp_line
		(start 3.15 5.35)
		(end 6 5.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "1f9968e1-0eee-4dd9-9f60-e366337fcb8a")
	)
	(fp_arc
		(start -3.15 3.5)
		(mid -3.032842 3.217158)
		(end -2.75 3.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "79a8ddb1-bca0-4377-810d-bba745d0d47a")
	)
	(fp_arc
		(start 2.75 3.1)
		(mid 3.032843 3.217157)
		(end 3.15 3.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "fe3354f4-538b-4062-a2ed-7998da18de18")
	)
	(fp_line
		(start -6.25 -7.95)
		(end -6.25 4.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e37c8ee8-778f-4fb1-a382-58b7f13327aa")
	)
	(fp_line
		(start -6.25 4.75)
		(end -3.25 4.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ff22bc1d-7252-46c8-aa56-2fcf3b0aed98")
	)
	(fp_line
		(start -3.25 4.75)
		(end -3.25 6.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d9f9bc89-eae5-48cd-8b86-84d6abf51ccf")
	)
	(fp_line
		(start -3.25 6.55)
		(end 3.25 6.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "518d3713-0903-49d2-b864-26e173b8a0f9")
	)
	(fp_line
		(start 3.25 4.75)
		(end 6.25 4.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f84130ff-a1e0-4834-9cae-bfae1372f93a")
	)
	(fp_line
		(start 3.25 6.55)
		(end 3.25 4.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ed8ec206-fcda-446a-9175-18a5c3a8bbe7")
	)
	(fp_line
		(start 6.25 -7.95)
		(end -6.25 -7.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e5bc91ed-6863-431b-8065-13df5a5a19bf")
	)
	(fp_line
		(start 6.25 4.5)
		(end 6.25 -7.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8a1bbd25-8cbb-424a-9b43-5d9e23660e59")
	)
	(fp_line
		(start 6.25 4.75)
		(end 6.25 4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fea8efb1-2ef5-475a-af92-65909d0f7abe")
	)
	(fp_line
		(start -6 -7.7)
		(end 6 -7.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d3c3fba2-2c99-4639-82b3-def615a0a111")
	)
	(fp_line
		(start -6 3.3)
		(end -6 -7.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "67f0fbee-d2a9-4d1e-b5f5-53c6e26db37e")
	)
	(fp_line
		(start -4.5 3.3)
		(end -6 3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6c9e6964-8f4f-4037-9cfa-40ec74f90ccb")
	)
	(fp_line
		(start -4.5 4.5)
		(end -4.5 3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d2eed008-515f-4d80-8797-64a02ee1a5fb")
	)
	(fp_line
		(start -4.5 4.5)
		(end -3 4.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "433d632b-1af0-4c6d-b40c-06543e114522")
	)
	(fp_line
		(start -3 4.5)
		(end -3 6.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "60c30c46-20da-47d2-8dde-e79a9730c8eb")
	)
	(fp_line
		(start -3 6.3)
		(end 3 6.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "290850ed-73e2-4ba6-869e-4fef127cbb88")
	)
	(fp_line
		(start 3 4.5)
		(end 3 6.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3498781e-a632-473a-8750-c7318af73043")
	)
	(fp_line
		(start 4.5 3.3)
		(end 6 3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9f408fd4-cdec-42a6-b29a-045b39095465")
	)
	(fp_line
		(start 4.5 4.5)
		(end 3 4.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8c470310-04d8-41c3-adc3-7a545498423f")
	)
	(fp_line
		(start 4.5 4.5)
		(end 4.5 3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a299908d-8fba-44bb-b5be-a7436df93aae")
	)
	(fp_line
		(start 6 3.3)
		(end 6 -7.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c692bdd3-7f87-4426-a4f0-4d6ad56edfad")
	)
	(fp_text user "PCB edge"
		(at 0 6.3 0)
		(unlocked yes)
		(layer "Dwgs.User")
		(uuid "280aa230-a25f-414c-9d84-47f182621149")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.5 0)
		(layer "F.Fab")
		(uuid "085988cb-9879-4ac3-a25a-5a2bd7285627")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -5 0)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "2a6783be-49b7-4a5e-8837-fde4f5b6b326")
	)
	(pad "" np_thru_hole circle
		(at -5 2.5)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "43e28b64-3f22-4d06-a9d9-1a6cbaeb55e4")
	)
	(pad "" np_thru_hole circle
		(at 0 -5)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "c28e13f1-55b0-4023-8004-5c43f3cb0c59")
	)
	(pad "" np_thru_hole circle
		(at 5 0)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "a43ddcff-5f56-4ac9-9af6-caeb3e1e6b3b")
	)
	(pad "" np_thru_hole circle
		(at 5 2.5)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "0dcf70ee-cde7-482b-a3e5-44427c25dbc7")
	)
	(pad "R" thru_hole oval
		(at -5 -5)
		(size 1.2 2.2)
		(drill oval 0.4 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e54c28a1-dfb5-4e3f-8b5a-7dd641ca7f3c")
	)
	(pad "RN" thru_hole oval
		(at -2.5 -5)
		(size 1.6 2.3)
		(drill oval 0.8 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "02b5eb1d-379e-426e-a14c-f52b3a21405a")
	)
	(pad "S" thru_hole oval
		(at 0 0)
		(size 2.2 1.2)
		(drill oval 1.4 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3ed7e64f-b114-42be-9bef-9a493d918a48")
	)
	(pad "T" thru_hole oval
		(at 5 -5 180)
		(size 1.2 2.2)
		(drill oval 0.4 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9fc83e1c-4425-4cec-92d0-a925a45db0ce")
	)
	(pad "TN" thru_hole oval
		(at 2.5 -5 180)
		(size 1.6 2.5)
		(drill oval 0.8 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1e85fd63-1943-4c11-8b94-66b8fbf95e55")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3525N_Horizontal.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
