# MikroTik RouterOS Patch  [[English](README_EN.md)]


### 国内镜像下载 密码: elseif
[ [123pan](https://www.123pan.com/s/IpxgTd-BYjQh.html) ]
[ [7.15.2](https://elseif.lanzouj.com/b00crdq4hg)]
[ [7.16beta4](https://elseif.lanzouj.com/b00crdq4fe) ] 
[ [7.15.2-arm64](https://elseif.lanzouj.com/b00crdq4ih) ] 
[ [7.16beta4-arm64](https://elseif.lanzouj.com/b00crdq4gf) ] 
[ [6.49.15](https://elseif.lanzouj.com/b00crdq4ji) ] 
[ [6.49.13](https://elseif.lanzouj.com/b00crdq4kj) ]       



![](image/install.png)
![](image/routeros.png)

### x86模式授权许可
![](image/x86.png)
### x86模式在线授权(v6.x)
![](image/renew_v6.png)
### Chr模式在线授权
![](image/renew.png)
### Chr模式授权许可
![](image/chr.png)

## 如何使用Shell
    安装 option-{version}.npk 包
    telnet到RouterOS,用户名devel,密码与admin的密码相同
## 如何授权许可
    进入shell
    运行 keygen
    参考上图。
    Chr镜像支持在线授权许可
## 如何使用Python
    安装 python3-{version}.npk 包
    telnet到RouterOS,用户名devel,密码与admin的密码相同
    运行 python -V
### npk.py
    对npk文件进行解包，修改，创建，签名和验证
### patch.py
    替换公钥并签名


## 所有的修补操作都自动运行在[Github Action](https://github.com/elseif/MikroTikPatch/blob/main/.github/workflows/)。





