From 168ef0c1dee83c401896a0bca680e9f97b1ebd64 Mon Sep 17 00:00:00 2001
From: Lorenzo Bianconi <lorenzo@kernel.org>
Date: Tue, 4 Mar 2025 15:21:11 +0100
Subject: [PATCH 4/6] net: airoha: Increase max mtu to 9k

EN7581 SoC supports 9k maximum MTU.

Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
Reviewed-by: Simon Horman <horms@kernel.org>
Link: https://patch.msgid.link/20250304-airoha-eth-rx-sg-v1-4-283ebc61120e@kernel.org
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/airoha/airoha_eth.h | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/airoha/airoha_eth.h
+++ b/drivers/net/ethernet/airoha/airoha_eth.h
@@ -20,7 +20,7 @@
 #define AIROHA_MAX_DSA_PORTS		7
 #define AIROHA_MAX_NUM_RSTS		3
 #define AIROHA_MAX_NUM_XSI_RSTS		5
-#define AIROHA_MAX_MTU			2000
+#define AIROHA_MAX_MTU			9216
 #define AIROHA_MAX_PACKET_SIZE		2048
 #define AIROHA_NUM_QOS_CHANNELS		4
 #define AIROHA_NUM_QOS_QUEUES		8
