From 5bbcda7576cd2bfa1ca8eaf415593a996da24c52 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Wed, 13 Feb 2019 12:33:29 +0000
Subject: [PATCH] staging: mmal_vchiq: Add in the Bayer encoding formats

The list of formats was copied before Bayer support was added.
The ISP supports Bayer and is being supported by the bcm2835_codec
driver, so add in the encodings for them.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 .../vc04_services/vchiq-mmal/mmal-encodings.h | 27 +++++++++++++++++++
 1 file changed, 27 insertions(+)

--- a/drivers/staging/vc04_services/vchiq-mmal/mmal-encodings.h
+++ b/drivers/staging/vc04_services/vchiq-mmal/mmal-encodings.h
@@ -69,6 +69,33 @@
  */
 #define MMAL_ENCODING_OPAQUE           MMAL_FOURCC('O', 'P', 'Q', 'V')
 
+/* Bayer formats
+ * FourCC values copied from V4L2 where defined.
+ */
+/* 8 bit per pixel Bayer formats. */
+#define MMAL_ENCODING_BAYER_SBGGR8     MMAL_FOURCC('B', 'A', '8', '1')
+#define MMAL_ENCODING_BAYER_SGBRG8     MMAL_FOURCC('G', 'B', 'R', 'G')
+#define MMAL_ENCODING_BAYER_SGRBG8     MMAL_FOURCC('G', 'R', 'B', 'G')
+#define MMAL_ENCODING_BAYER_SRGGB8     MMAL_FOURCC('R', 'G', 'G', 'B')
+
+/* 10 bit per pixel packed Bayer formats. */
+#define MMAL_ENCODING_BAYER_SBGGR10P   MMAL_FOURCC('p', 'B', 'A', 'A')
+#define MMAL_ENCODING_BAYER_SGRBG10P   MMAL_FOURCC('p', 'g', 'A', 'A')
+#define MMAL_ENCODING_BAYER_SGBRG10P   MMAL_FOURCC('p', 'G', 'A', 'A')
+#define MMAL_ENCODING_BAYER_SRGGB10P   MMAL_FOURCC('p', 'R', 'A', 'A')
+
+/* 12 bit per pixel packed Bayer formats. */
+#define MMAL_ENCODING_BAYER_SBGGR12P   MMAL_FOURCC('p', 'B', '1', '2')
+#define MMAL_ENCODING_BAYER_SGRBG12P   MMAL_FOURCC('p', 'g', '1', '2')
+#define MMAL_ENCODING_BAYER_SGBRG12P   MMAL_FOURCC('p', 'G', '1', '2')
+#define MMAL_ENCODING_BAYER_SRGGB12P   MMAL_FOURCC('p', 'R', '1', '2')
+
+/* 16 bit per pixel Bayer formats. */
+#define MMAL_ENCODING_BAYER_SBGGR16    MMAL_FOURCC('B', 'G', '1', '6')
+#define MMAL_ENCODING_BAYER_SGBRG16    MMAL_FOURCC('G', 'B', '1', '6')
+#define MMAL_ENCODING_BAYER_SGRBG16    MMAL_FOURCC('G', 'R', '1', '6')
+#define MMAL_ENCODING_BAYER_SRGGB16    MMAL_FOURCC('R', 'G', '1', '6')
+
 /** An EGL image handle
  */
 #define MMAL_ENCODING_EGL_IMAGE        MMAL_FOURCC('E', 'G', 'L', 'I')
