From 8f1b61ea1cb98735aa15a8875d729c21a2169fb9 Mon Sep 17 00:00:00 2001
From: Devi Priya <quic_devipriy@quicinc.com>
Date: Thu, 13 Mar 2025 16:33:59 +0530
Subject: [PATCH 22/22] v6.15: arm64: defconfig: Build NSS Clock Controller
 driver for IPQ9574

NSSCC driver is needed to enable the ethernet interfaces present
in RDP433 based on IPQ9574. Since this is not necessary for bootup
enabling it as a module.

Reviewed-by: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Signed-off-by: Devi Priya <quic_devipriy@quicinc.com>
Signed-off-by: Manikanta Mylavarapu <quic_mmanikan@quicinc.com>
Link: https://lore.kernel.org/r/20250313110359.242491-7-quic_mmanikan@quicinc.com
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
---
 arch/arm64/configs/defconfig | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/arm64/configs/defconfig
+++ b/arch/arm64/configs/defconfig
@@ -1312,6 +1312,7 @@ CONFIG_IPQ_GCC_5332=y
 CONFIG_IPQ_GCC_6018=y
 CONFIG_IPQ_GCC_8074=y
 CONFIG_IPQ_GCC_9574=y
+CONFIG_IPQ_NSSCC_9574=m
 CONFIG_MSM_GCC_8916=y
 CONFIG_MSM_MMCC_8994=m
 CONFIG_MSM_GCC_8994=y
