From 690e2d40fe645e86dcd0ac265038426676473e19 Mon Sep 17 00:00:00 2001
From: Matteo Croce <technoboy85@gmail.com>
Date: Fri, 21 May 2021 03:26:38 +0200
Subject: [PATCH 1011/1021] net: stmmac: use GFP_DMA32

Signed-off-by: Matteo Croce <mcroce@microsoft.com>
---
 drivers/net/ethernet/stmicro/stmmac/stmmac_main.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/net/ethernet/stmicro/stmmac/stmmac_main.c
+++ b/drivers/net/ethernet/stmicro/stmmac/stmmac_main.c
@@ -1460,7 +1460,7 @@ static int stmmac_init_rx_buffers(struct
 {
 	struct stmmac_rx_queue *rx_q = &dma_conf->rx_queue[queue];
 	struct stmmac_rx_buffer *buf = &rx_q->buf_pool[i];
-	gfp_t gfp = (GFP_ATOMIC | __GFP_NOWARN);
+	gfp_t gfp = (GFP_ATOMIC | __GFP_NOWARN | GFP_DMA32);
 
 	if (priv->dma_cap.host_dma_width <= 32)
 		gfp |= GFP_DMA32;
@@ -4791,7 +4791,7 @@ static inline void stmmac_rx_refill(stru
 	struct stmmac_rx_queue *rx_q = &priv->dma_conf.rx_queue[queue];
 	int dirty = stmmac_rx_dirty(priv, queue);
 	unsigned int entry = rx_q->dirty_rx;
-	gfp_t gfp = (GFP_ATOMIC | __GFP_NOWARN);
+	gfp_t gfp = (GFP_ATOMIC | __GFP_NOWARN | GFP_DMA32);
 
 	if (priv->dma_cap.host_dma_width <= 32)
 		gfp |= GFP_DMA32;
