From 850f785a1f8c8448db4d70983595b2b088cf60b7 Mon Sep 17 00:00:00 2001
From: Anton Vorontsov <avorontsov@ru.mvista.com>
Date: Fri, 16 Oct 2009 20:47:22 +0400
Subject: [PATCH] powerpc/83xx: Fix u-boot partion size for MPC8377E-WLAN boards

u-boot partition size should be 0x80000 (512 KB), not 0x8000 (32 KB).

Signed-off-by: Anton Vorontsov <avorontsov@ru.mvista.com>
Signed-off-by: Kumar Gala <galak@kernel.crashing.org>
---
 arch/powerpc/boot/dts/mpc8377_wlan.dts |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

--- a/arch/powerpc/boot/dts/mpc8377_wlan.dts
+++ b/arch/powerpc/boot/dts/mpc8377_wlan.dts
@@ -67,7 +67,7 @@
 			device-width = <1>;
 
 			partition@0 {
-				reg = <0 0x8000>;
+				reg = <0 0x80000>;
 				label = "u-boot";
 				read-only;
 			};
