From 423d67db899b8f2e20b09fac7da1f7eaaa4523cb Mon Sep 17 00:00:00 2001
From: Kurt Mahan <kmahan@freescale.com>
Date: Tue, 24 Jun 2008 23:24:30 -0600
Subject: [PATCH] Add the M547x/M548x NOR_FLASH base address.

LTIBName: m547x-8x-NOR-FLASH-baseaddr
Signed-off-by: Kurt Mahan <kmahan@freescale.com>
---
 arch/m68k/Kconfig |    1 +
 1 files changed, 1 insertions(+), 0 deletions(-)

--- a/arch/m68k/Kconfig
+++ b/arch/m68k/Kconfig
@@ -459,6 +459,7 @@ config NOR_FLASH_BASE
 	depends on COLDFIRE
 	default 0x00000000 if M54451EVB
 	default 0x00000000 if M54455EVB
+	default 0xE0000000 if M547X_8X
 
 config M68KFPU_EMU
 	bool "Math emulation support (EXPERIMENTAL)"
